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	Handheld Through-the-Wall Radar Life Detector
	GA700


Description
This ultra-portable tactical device leverages advanced Ultra-Wideband (UWB) and Stepped-Frequency Continuous Wave (SFCW) radar technology to penetrate non-metallic barriers such as brick, concrete, and wooden structures. It enables real-time, non-contact detection and monitoring of living subjects hidden behind walls, providing operators with immediate feedback on human presence, distance, and subtle movements like breathing. With robust signal processing algorithms, the system maintains high detection accuracy and minimal false alarms even in complex, cluttered environments.

Weighing only 1.3 kg and featuring an intuitive interface, the radar supports flexible operational modes including stand-off scanning and synchronized multi-unit deployment. It is an essential tool for military reconnaissance, counter-terrorism operations, law enforcement raids, and emergency rescue missions. By delivering critical situational awareness and revealing concealed threats, the device empowers personnel to execute missions with enhanced safety, precision, and operational confidence.
[bookmark: OLE_LINK1]Features
· Compact and Lightweight: Weighs only 1.3 kg.
· High Penetration Capability: Can effectively penetrate solid brick walls up to 50 cm thick.
· Long Detection Range: Detection distance up to 30 meters.
· Excellent Detection Performance: High detection accuracy with low false alarm rate.
· Non-Contact Operation: Can detect without direct contact with the wall.
· Multi-Device Synchronous Operation: Multiple units can operate simultaneously without mutual interference.
· Wireless Remote Control: Supports wireless remote operation.
Applications
· Hostage Rescue
· Counter-terrorism Operations
· Urban Warfare / Urban Operations
· Intelligence Gathering
· Reconnaissance and Surveillance
· High-risk Apprehension / Tactical Arrest
· Narcotics Enforcement Operations
· Search and Rescue Operations
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1. Parameter
	Device Type
	Handheld Through-the-Wall Life Detection Radar

	Maximum Penetration Thickness
	Brick wall: ≥ 50 cm

	Number of Walls Penetrable
	No less than 2 walls

	Maximum Detection Range
	Static Target： ≥ 25 m

	
	Moving Target： ≥ 30 m

	Maximum Number of Targets
	3

	Detection Angle
	Azimuth and elevation angle not less than 100°

	Display Screen
	Color LCD

	Display Mode
	Graphic + Text + Numeric Values

	Target Information
	Target presence, number of targets, target distance, detection time

	Resolution
	Better than 0.3 m

	Power Supply Method
	Rechargeable Lithium-Ion Battery

	Battery Endurance Time
	Not less than 4 hours

	[bookmark: _GoBack]Wireless Functionality
	Yes

	Temperature
	Operating Temperature: -20°C to +55°C
Storage Temperature: -40°C to +60°C

	Dustproof & Waterproof
	IP65

	Dimensions
	Length: 227mm, Width: 108mm, Thickness: 105mm

	Weight
	1.3 kg



2. Packing List
	No.
	Item
	Quantity
	Optional 

	1
	GA700 Handheld Through-Wall Radar Life Detector
	1 unit
	Standard 

	2
	Charger
	1 set
	Standard 
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